!   Commands inserted into this file will be executed just after material definitions in /PREP7.
!   The material number for this body is equal to the parameter "matid".

!   Active UNIT system in Workbench when this object was created:  Metric (mm, kg, N, s, mV, mA)
!   NOTE:  Any data that requires units (such as mass) is assumed to be in the consistent solver unit system.
!                See Solving Units in the help system for more information.


! --------------
! Set parameters
! --------------

e = 100000         ! Young's modulus
nupl = 0.03        ! Plastic Poisson's ratio in tension

epsy_t = 0.055E-2  ! Strain value at yielding in tension
epsy_c = 0.203E-2  ! Strain value at yielding in compression

sigy_t = e*epsy_t  ! Stress value at yielding in tension
sigy_c = e*epsy_c  ! Stress value at yielding in compression


! ----------------------
! Define cast-iron model
! ----------------------

tb,cast,matid,,,isotropic
tbdata,1,nupl

tb,uniaxial,matid,1,5,tension
tbpt,,epsy_t,sigy_t
tbpt,,0.10E-02,90
tbpt,,0.25E-02,166
tbpt,,0.35E-02,199
tbpt,,0.45E-02,222

tb,uniaxial,matid,1,5,compression
tbpt,,epsy_c,sigy_c
tbpt,,0.50E-02,345
tbpt,,0.80E-02,401
tbpt,,1.10E-02,453
tbpt,,1.40E-02,483

! ------------------------
! List material properties
! ------------------------

mplist,matid
tblist,all,matid 