cmsel,s,pressure	!Named selection represents all nodes on lower half of seal face
esln,s,1		!select elements attached to nodes
esel,r,type,,cid_1	!reselect only the contact elements with type 'cid_1'
!
sfe,all,1,pres,,50	!apply fluid pressure of 50Mpa to selected contact elements
!
cmsel,s,start_pt	!select starting point
esln
esel,r,type,,cid_1	!reselect only contact element attached to starting point
sfe,all,2,pres,,1	!specify the above location to be initially exposed to fluid pressure
!
allsel			!reselect all elements