<?xml version="1.0" encoding="UTF-8"?>
<ANSYS_EnggData version="2">
	<ParameterData id="57c07e22-8b92-42bb-a684-ec063ca99e7f"/>
	<MaterialData>
		<Sources>
			<Source>
				<MaterialName>Structural Steel</MaterialName>
				<NameInSource>Structural Steel</NameInSource>
				<Location>C:\Program Files\ANSYS Inc\v110\AISOL\CommonFiles\Language\en-us\EngineeringData\Materials\Workbench_Samples.xml</Location>
			</Source>
		</Sources>
		<MatML_Doc>
			<Material>
				<BulkDetails>
					<Name>Structural Steel</Name>
					<PropertyData property="pr1">
						<Data format="float">0.</Data>
						<Qualifier>Compressive Ultimate Strength</Qualifier>
					</PropertyData>
					<PropertyData property="pr2">
						<Data format="float">250000000.</Data>
						<Qualifier>Compressive Yield Strength</Qualifier>
					</PropertyData>
					<PropertyData property="pr3">
						<Data format="float">7850.</Data>
						<Qualifier>Density</Qualifier>
						<ParameterValue parameter="pa1" format="float">7.88860905221012e-031</ParameterValue>
					</PropertyData>
					<PropertyData property="pr4">
						<Data format="float">0.2</Data>
						<Qualifier>Ductility</Qualifier>
					</PropertyData>
					<PropertyData property="pr5">
						<Data format="float">0.3</Data>
						<Qualifier>Poisson's Ratio</Qualifier>
						<ParameterValue parameter="pa2" format="float">7.88860905221012e-031</ParameterValue>
					</PropertyData>
					<PropertyData property="pr6">
						<Data format="float">250000000.</Data>
						<Qualifier>Tensile Yield Strength</Qualifier>
					</PropertyData>
					<PropertyData property="pr7">
						<Data format="float">460000000.</Data>
						<Qualifier>Tensile Ultimate Strength</Qualifier>
					</PropertyData>
					<PropertyData property="pr8">
						<Data format="float">200000000000.</Data>
						<Qualifier>Young's Modulus</Qualifier>
						<ParameterValue parameter="pa3" format="float">7.88860905221012e-031</ParameterValue>
					</PropertyData>
					<PropertyData property="pr9">
						<Data format="float">1.2e-005</Data>
						<Qualifier>Thermal Expansion</Qualifier>
						<ParameterValue parameter="pa4" format="float">7.88860905221012e-031</ParameterValue>
					</PropertyData>
					<PropertyData property="pr10">
						<Data format="float">434.</Data>
						<Qualifier>Specific Heat</Qualifier>
						<ParameterValue parameter="pa5" format="float">7.88860905221012e-031</ParameterValue>
					</PropertyData>
					<PropertyData property="pr11">
						<Data format="float">60.5</Data>
						<Qualifier>Thermal Conductivity</Qualifier>
						<ParameterValue parameter="pa6" format="float">21.</ParameterValue>
					</PropertyData>
					<PropertyData property="pr12" technique="mt1">
						<Data format="float">3999000000.,2827000000.,1896000000.,1413000000.,1069000000.,441000000.,262000000.,214000000.,138000000.,114000000.,86200000.</Data>
						<Qualifier>Alternating Stress</Qualifier>
						<ParameterValue parameter="pa7" format="float">10.,20.,50.,100.,200.,2000.,10000.,20000.,100000.,200000.,1000000.</ParameterValue>
						<ParameterValue parameter="pa8" format="float">0.,0.,0.,0.,0.,0.,0.,0.,0.,0.,0.</ParameterValue>
					</PropertyData>
					<PropertyData property="pr13" technique="mt2">
						<Data format="float">920000000.</Data>
						<Qualifier>Strength Coefficient</Qualifier>
					</PropertyData>
					<PropertyData property="pr13" technique="mt3">
						<Data format="float">-0.106</Data>
						<Qualifier>Strength Exponent</Qualifier>
					</PropertyData>
					<PropertyData property="pr13" technique="mt4">
						<Data format="float">0.213</Data>
						<Qualifier>Ductility Coefficient</Qualifier>
					</PropertyData>
					<PropertyData property="pr13" technique="mt5">
						<Data format="float">-0.47</Data>
						<Qualifier>Ductility Exponent</Qualifier>
					</PropertyData>
					<PropertyData property="pr13" technique="mt6">
						<Data format="float">1000000000.</Data>
						<Qualifier>Cyclic Strength Coefficient</Qualifier>
					</PropertyData>
					<PropertyData property="pr13" technique="mt7">
						<Data format="float">0.2</Data>
						<Qualifier>Cyclic Strain Hardening Exponent</Qualifier>
					</PropertyData>
					<PropertyData property="pr14">
						<Data format="float">10000.</Data>
						<Qualifier>Relative Permeability</Qualifier>
					</PropertyData>
					<PropertyData property="pr15">
						<Data format="float">1.7e-007</Data>
						<Qualifier>Resistivity</Qualifier>
					</PropertyData>
				</BulkDetails>
				<Metadata>
					<PropertyDetails id="pr1">
						<Name>Compressive Ultimate Strength</Name>
					</PropertyDetails>
					<PropertyDetails id="pr2">
						<Name>Compressive Yield Strength</Name>
					</PropertyDetails>
					<ParameterDetails id="pa1">
						<Name>Temperature</Name>
					</ParameterDetails>
					<PropertyDetails id="pr3">
						<Name>Density</Name>
					</PropertyDetails>
					<PropertyDetails id="pr4">
						<Name>Ductility</Name>
					</PropertyDetails>
					<ParameterDetails id="pa2">
						<Name>Temperature</Name>
					</ParameterDetails>
					<PropertyDetails id="pr5">
						<Name>Poisson's Ratio</Name>
					</PropertyDetails>
					<PropertyDetails id="pr6">
						<Name>Tensile Yield Strength</Name>
					</PropertyDetails>
					<PropertyDetails id="pr7">
						<Name>Tensile Ultimate Strength</Name>
					</PropertyDetails>
					<ParameterDetails id="pa3">
						<Name>Temperature</Name>
					</ParameterDetails>
					<PropertyDetails id="pr8">
						<Name>Young's Modulus</Name>
					</PropertyDetails>
					<ParameterDetails id="pa4">
						<Name>Temperature</Name>
					</ParameterDetails>
					<PropertyDetails id="pr9">
						<Name>Thermal Expansion</Name>
					</PropertyDetails>
					<ParameterDetails id="pa5">
						<Name>Temperature</Name>
					</ParameterDetails>
					<PropertyDetails id="pr10">
						<Name>Specific Heat</Name>
					</PropertyDetails>
					<ParameterDetails id="pa6">
						<Name>Temperature</Name>
					</ParameterDetails>
					<PropertyDetails id="pr11">
						<Name>Thermal Conductivity</Name>
					</PropertyDetails>
					<MeasurementTechniqueDetails id="mt1">
						<Name>Log-Log</Name>
					</MeasurementTechniqueDetails>
					<ParameterDetails id="pa7">
						<Name>Cycles</Name>
					</ParameterDetails>
					<ParameterDetails id="pa8">
						<Name>Mean Stress</Name>
					</ParameterDetails>
					<PropertyDetails id="pr12">
						<Name>Alternating Stress</Name>
					</PropertyDetails>
					<MeasurementTechniqueDetails id="mt2">
						<Name>Strain-Life</Name>
					</MeasurementTechniqueDetails>
					<MeasurementTechniqueDetails id="mt3">
						<Name>Strain-Life</Name>
					</MeasurementTechniqueDetails>
					<MeasurementTechniqueDetails id="mt4">
						<Name>Strain-Life</Name>
					</MeasurementTechniqueDetails>
					<MeasurementTechniqueDetails id="mt5">
						<Name>Strain-Life</Name>
					</MeasurementTechniqueDetails>
					<MeasurementTechniqueDetails id="mt6">
						<Name>Strain-Life</Name>
					</MeasurementTechniqueDetails>
					<MeasurementTechniqueDetails id="mt7">
						<Name>Strain-Life</Name>
					</MeasurementTechniqueDetails>
					<PropertyDetails id="pr13">
						<Name>Strain-Life Parameters</Name>
					</PropertyDetails>
					<PropertyDetails id="pr14">
						<Name>Relative Permeability</Name>
					</PropertyDetails>
					<PropertyDetails id="pr15">
						<Name>Resistivity</Name>
					</PropertyDetails>
				</Metadata>
			</Material>
		</MatML_Doc>
	</MaterialData>
	<ConvectionData>
		<Sources>
			<Source>
				<LoadVariationName>Stagnant Air - Simplified Case</LoadVariationName>
				<NameInSource>Stagnant Air - Simplified Case</NameInSource>
				<Location>C:\Program Files\ANSYS Inc\v110\AISOL\CommonFiles\Language\en-us\EngineeringData\Materials\Workbench_Samples.xml</Location>
			</Source>
		</Sources>
		<MatML_Doc>
			<LoadVariation>
				<BulkDetails>
					<Name>Stagnant Air - Simplified Case</Name>
					<PropertyData property="pr1" technique="mt1">
						<Data format="float">5.</Data>
						<Qualifier>Convection Coefficient</Qualifier>
						<ParameterValue parameter="pa1" format="float">21.</ParameterValue>
					</PropertyData>
				</BulkDetails>
				<Metadata>
					<MeasurementTechniqueDetails id="mt1">
						<Name>Average Film Temperature</Name>
					</MeasurementTechniqueDetails>
					<ParameterDetails id="pa1">
						<Name>Temperature</Name>
					</ParameterDetails>
					<PropertyDetails id="pr1">
						<Name>Convection Coefficient</Name>
					</PropertyDetails>
				</Metadata>
			</LoadVariation>
		</MatML_Doc>
	</ConvectionData>
	<LoadVariationData>
		<Sources>
			<Source>
				<LoadVariationName>Moment vs. Time</LoadVariationName>
				<NameInSource/>
				<Location></Location>
			</Source>
		</Sources>
		<MatML_Doc>
			<LoadVariation>
				<BulkDetails>
					<Name>Moment vs. Time</Name>
					<PropertyData property="pr1">
						<Data format="float">0.,5.</Data>
						<Qualifier>Moment</Qualifier>
						<ParameterValue parameter="pa1" format="float">0.,60.</ParameterValue>
					</PropertyData>
				</BulkDetails>
				<Metadata>
					<ParameterDetails id="pa1">
						<Name>Time</Name>
					</ParameterDetails>
					<PropertyDetails id="pr1">
						<Name>Moment</Name>
					</PropertyDetails>
				</Metadata>
			</LoadVariation>
		</MatML_Doc>
	</LoadVariationData>
	<BeamSectionData>
		<Sources/>
		<MatML_Doc/>
	</BeamSectionData>
</ANSYS_EnggData>
