!   Commands inserted into this file will be executed just after material definitions in /PREP7.
!   The material number for this body is equal to the parameter "matid".

!   Active UNIT system in Workbench when this object was created:  Metric (mm, kg, N, s, mV, mA)
!   NOTE:  Any data that requires units (such as mass) is assumed to be in the consistent solver unit system.
!                See Solving Units in the help system for more information.


!---------------------------------------
! Define Hill material properties
!---------------------------------------
 
tb,hill,matid        
tbdata,1,1.10 ! Yield stress ratio in  X direction
tbdata,2,1.10 ! Yield stress ratio in  Y direction
tbdata,3,1.00 ! Yield stress ratio in  Z direction
tbdata,4,1.00 ! Yield stress ratio in XY direction
tbdata,5,1.00 ! Yield stress ratio in YZ direction
tbdata,6,1.00 ! Yield stress ratio in XZ direction

tblist,all,all